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Color Match Information 

If you have any questions, please contact our Lab Technicians in the Color Lab @ 1-800-661-9930

	Date Received in Lab:          am/pm            
	Date Required: 

	Brought in to Lab By: 

	Customer Sample Received?     Yes      No 
	If yes) Returned? Yes         No

	What is Being Painted? Propane Haulers

	CLR#
	Gloss Level: 

	Does this color need to be lead free     YES     NO     Note:

	Description or Color Name: 

	If automotive:

	Model:
	Make:
	Year:
	Codes: (If available)

	
	
	
	

	Sizing Requirements
	
	
	
	

	Pint
	Quart
	Gallon
	Pail
	Fax formula to distributor #

	Company Name & Contact:

	Phone #

	Email:

	Is this a fleet color that will be bought repeatedly or just a “one-time” deal? 
	

	If it is a metallic/pearl color, do you want it matched as base/clear in O.E.M. fashion or a single stage?  
Most new pearl/metallic colors need to be base/clear for a “acceptable match”.
	

	Single stage and to some degree base/clear colors are application dependent and will change depending on the applicator/viscosity/and air pressure used.  We recommend using conventional spray at 40-45 psi. 
	

	Our paint colors are made to match in daylight conditions and may not match under other lights sources. 
	

	Note: Solid colors may require 24 hours to match. 
Pearls, medium-lo-no gloss and some metallics may take up to 5 working days to match.
O.E.M. touch-ups are not recommended – only complete paint jobs.

	
	

	Final Spectrophotometer Delta E (if applicable) =  
	

	Matched By: 
	



	Is this a corporate color that requires Official Color Standards  
	Yes            No

	Requested Color Name:
	Approved by:
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